if {![have_include power_on/qemu] || [have_spec foc] || [have_spec linux] ||
    [have_board rpi3] || [have_board imx53_qsb_tz]} {

	puts "Run script is not supported on this platform."
	exit 0
}

if {[get_cmd_switch --autopilot] && [have_board virt_qemu_riscv]} {
	puts "Autopilot mode is not supported on this platform."
	exit 0
}

create_boot_directory

import_from_depot [depot_user]/src/[base_src] \
                  [depot_user]/pkg/[drivers_nic_pkg]

build { app/ping server/nic_router init }

append config {

<config>

	<parent-provides>
		<service name="ROM"/>
		<service name="IRQ"/>
		<service name="IO_MEM"/>
		<service name="IO_PORT"/>
		<service name="PD"/>
		<service name="RM"/>
		<service name="CPU"/>
		<service name="LOG"/>
	</parent-provides>

	<default-route>
		<any-service> <parent/> <any-child/> </any-service>
	</default-route>

	<default caps="200"/>

	<start name="timer">
		<resource name="RAM" quantum="1M"/>
		<provides><service name="Timer"/></provides>
	</start>

	<start name="drivers" caps="1000" managing_system="yes">
		<resource name="RAM" quantum="32M"/>
		<binary name="init"/>
		<route>
			<service name="ROM" label="config"> <parent label="drivers.config"/> </service>
			<service name="Timer"> <child name="timer"/> </service>
			<service name="Uplink"> <child name="nic_router"/> </service>
			<any-service> <parent/> </any-service>
		</route>
	</start>

	<start name="nic_router">
		<resource name="RAM" quantum="10M"/>
		<provides>
			<service name="Nic"/>
			<service name="Uplink"/>
		</provides>
		<config>

			<policy label_prefix="ping"    domain="downlink"/>
			<policy label_prefix="drivers" domain="uplink"/>

			<domain name="uplink" use_arp="no" verbose_packets="yes">
				<nat domain="downlink" icmp-ids="100"/>
			</domain>

			<domain name="downlink" interface="10.0.3.1/24">
				<icmp dst="10.0.2.2/24" domain="uplink"/>
			</domain>

		</config>
	</start>

	<start name="ping">
		<resource name="RAM" quantum="8M"/>
		<config interface="10.0.3.2/24"
		        gateway="10.0.3.1"
		        dst_ip="10.0.2.2"
		        period_sec="1"
		        count="2"/>
		<route>
			<service name="Nic"> <child name="nic_router"/> </service>
			<any-service> <parent/> <any-child/> </any-service>
		</route>
	</start>

</config>}

install_config $config

build_boot_image { ping nic_router init }

append qemu_args " -nographic "
append_qemu_nic_args

set done_string ".*child \"ping\" exited with exit value 0.*\n"

run_genode_until $done_string 30

grep_output { ARP }
compare_output_to {}
