if {[expr ![have_spec nova] && ![have_spec sel4] && ![have_spec hw] && ![have_spec foc] || ![have_spec x86] || [have_include power_on/qemu]]} {
	puts "\n Run script is not supported on this platform. \n"; exit 0 }

proc wifi_ssid {} {
	return "$::env(GENODE_WIFI_SSID2)" }

proc wifi_psk {} {
	return "$::env(GENODE_WIFI_PSK2)" }

proc router_verbose {} {
	return "no" }

proc router_verbose_packet_drop {} {
	return "no" }

proc router_verbose_packets {} {
	return "no" }

proc router_verbose_domain_state {} {
	return "yes" }

source ${genode_dir}/repos/base/run/platform_drv.inc

proc platform_drv_priority {} { return { priority="-1"} }

append build_components { core }
append build_components { init }
append build_components { timer }
append build_components { server/nic_router }
append build_components { server/dynamic_rom }
append build_components { server/report_rom }
append build_components { drivers/wifi }
append build_components { lib/vfs/jitterentropy }
append build_components { drivers/rtc }
append build_components { drivers/nic }
append build_components { app/ping }

append_platform_drv_build_components

build $build_components

create_boot_directory

append config {

<config prio_levels="4">
	<parent-provides>
		<service name="ROM"/>
		<service name="IRQ"/>
		<service name="IO_MEM"/>
		<service name="IO_PORT"/>
		<service name="PD"/>
		<service name="RM"/>
		<service name="CPU"/>
		<service name="LOG"/>
	</parent-provides>
	<default-route>
		<any-service> <parent/> <any-child/> </any-service>
	</default-route>
	<default caps="100"/>}

append_platform_drv_config
append config {

	<start name="timer" priority="0">
		<resource name="RAM" quantum="1M"/>
		<provides><service name="Timer"/></provides>
	</start>

	<start name="rtc_drv" priority="-1">
		<resource name="RAM" quantum="1M"/>
		<provides>
			<service name="Rtc"/>
		</provides>
	</start>

	<start name="nic_drv" priority="-1" caps="120">
		<binary name="ipxe_nic_drv"/>
		<resource name="RAM" quantum="8M"/>
		<route>
			<service name="Uplink"> <child name="router"/> </service>
			<any-service> <parent/> <any-child/> </any-service>
		</route>
	</start>

	<start name="wifi_drv" caps="300" priority="-1">
		<resource name="RAM" quantum="24M"/>
		<config ld_verbose="no">
			<vfs>
				<dir name="dev"> <log/> <rtc/> <null/>
					<jitterentropy name="random"/>
					<jitterentropy name="urandom"/>
				</dir>
				<dir name="config"> <ram/> </dir>
			</vfs>
			<libc stdout="/dev/null" stderr="/dev/null" rtc="/dev/rtc"/>
		</config>
		<route>
			<service name="Uplink"> <child name="router"/> </service>
			<service name="Rtc"> <any-child/> </service>
			<service name="Report"> <child name="report_rom"/> </service>
			<service name="ROM" label="wifi_config"> <child name="config_rom"/> </service>
			<any-service> <parent/> <any-child/> </any-service>
		</route>
	</start>

	<start name="report_rom" priority="-2">
		<resource name="RAM" quantum="2M"/>
		<provides> <service name="Report"/> <service name="ROM"/> </provides>
		<config/>
	</start>

	<start name="config_rom" priority="-2">
		<binary name="dynamic_rom"/>
		<resource name="RAM" quantum="4M"/>
		<provides><service name="ROM"/></provides>
		<config verbose="no">
			<rom name="wifi_config">
				<inline description="CONNECT">
<wifi_config connected_scan_interval="0" scan_interval="5" rfkill="no" verbose="no" verbose_state="no">
   <network ssid="} [wifi_ssid] {" protection="WPA2" passphrase="} [wifi_psk] {"/>
</wifi_config>
				</inline>
				<sleep milliseconds="600000"/> <!-- 10 minutes -->
			</rom>
		</config>
	</start>

	<start name="dynamic_rom" priority="-1">
		<resource name="RAM" quantum="4M"/>
		<provides><service name="ROM"/> </provides>
		<config verbose="yes">
			<rom name="router.config">

				<!-- give the drivers time to come up -->
				<inline> <config/> </inline>
				<sleep milliseconds="15000"/>

				<!-- start the actual test -->
				<inline>

					<config dhcp_discover_timeout_sec="1"
					        verbose="}              [router_verbose] {"
					        verbose_packet_drop="}  [router_verbose_packet_drop] {"
					        verbose_domain_state="} [router_verbose_domain_state] {"
					        verbose_packets="}      [router_verbose_packets] {">

						<policy label_prefix="ping"    domain="downlink"/>
						<policy label_prefix="nic_drv" domain="uplink"  />

						<domain name="uplink">
							<nat domain="downlink" icmp-ids="999"/>
						</domain>

						<domain name="downlink" interface="10.0.1.79/24">
							<dhcp-server ip_first="10.0.1.80" ip_last="10.0.1.100"/>
							<icmp dst="0.0.0.0/0" domain="uplink" />
						</domain>

					</config>

				</inline>
				<sleep milliseconds="3001"/>
				<inline>

					<config dhcp_discover_timeout_sec="1"
					        verbose="}              [router_verbose] {"
					        verbose_packet_drop="}  [router_verbose_packet_drop] {"
					        verbose_domain_state="} [router_verbose_domain_state] {"
					        verbose_packets="}      [router_verbose_packets] {">

						<policy label_prefix="ping"     domain="downlink"/>
						<policy label_prefix="wifi_drv" domain="uplink"  />

						<domain name="uplink">
							<nat domain="downlink" icmp-ids="999"/>
						</domain>

						<domain name="downlink" interface="10.0.1.79/24">
							<dhcp-server ip_first="10.0.1.80" ip_last="10.0.1.100"/>
							<icmp dst="0.0.0.0/0" domain="uplink" />
						</domain>

					</config>

				</inline>
				<sleep milliseconds="3002"/>
				<inline>

					<config dhcp_discover_timeout_sec="1"
					        verbose="yes"
					        verbose_packet_drop="}  [router_verbose_packet_drop] {"
					        verbose_domain_state="} [router_verbose_domain_state] {"
					        verbose_packets="}      [router_verbose_packets] {">

						<policy label_prefix="ping" domain="downlink"/>

						<domain name="downlink" interface="10.0.1.79/24">
							<dhcp-server ip_first="10.0.1.80" ip_last="10.0.1.100"/>
							<icmp dst="0.0.0.0/0" domain="uplink" />
						</domain>

					</config>

				</inline>
				<sleep milliseconds="3003"/>
				<inline>

					<config dhcp_discover_timeout_sec="1"
					        verbose="}              [router_verbose] {"
					        verbose_packet_drop="}  [router_verbose_packet_drop] {"
					        verbose_domain_state="} [router_verbose_domain_state] {"
					        verbose_packets="}      [router_verbose_packets] {">

						<policy label_prefix="ping"    domain="downlink"/>
						<policy label_prefix="nic_drv" domain="uplink"  />

						<domain name="uplink">
							<nat domain="downlink" icmp-ids="999"/>
						</domain>

						<domain name="downlink" interface="10.0.1.79/24">
							<dhcp-server ip_first="10.0.1.80" ip_last="10.0.1.100"/>
							<icmp dst="0.0.0.0/0" domain="uplink" />
						</domain>

					</config>

				</inline>
				<sleep milliseconds="3004"/>
				<inline>

					<config dhcp_discover_timeout_sec="1"
					        verbose="}              [router_verbose] {"
					        verbose_packet_drop="}  [router_verbose_packet_drop] {"
					        verbose_domain_state="} [router_verbose_domain_state] {"
					        verbose_packets="}      [router_verbose_packets] {">

						<policy label_prefix="ping"    domain="downlink"/>
						<policy label_prefix="nic_drv" domain="uplink"  />

						<domain name="uplink">
							<nat domain="downlink" icmp-ids="999"/>
						</domain>

						<domain name="downlink" interface="10.0.1.79/24">
							<dhcp-server ip_first="10.0.1.80" ip_last="10.0.1.100"/>
							<icmp dst="0.0.0.0/0" domain="uplink" />
						</domain>

					</config>

				</inline>
				<sleep milliseconds="3005"/>
				<inline>

					<config dhcp_discover_timeout_sec="1"
					        verbose="yes"
					        verbose_packet_drop="}  [router_verbose_packet_drop] {"
					        verbose_domain_state="} [router_verbose_domain_state] {"
					        verbose_packets="}      [router_verbose_packets] {">

						<policy label_prefix="ping" domain="downlink"/>

						<domain name="downlink" interface="10.0.1.79/24">
							<dhcp-server ip_first="10.0.1.80" ip_last="10.0.1.100"/>
							<icmp dst="0.0.0.0/0" domain="uplink" />
						</domain>

					</config>

				</inline>
				<sleep milliseconds="3006"/>
				<inline>

					<config dhcp_discover_timeout_sec="1"
					        verbose="}              [router_verbose] {"
					        verbose_packet_drop="}  [router_verbose_packet_drop] {"
					        verbose_domain_state="} [router_verbose_domain_state] {"
					        verbose_packets="}      [router_verbose_packets] {">

						<policy label_prefix="ping"     domain="downlink"/>
						<policy label_prefix="wifi_drv" domain="uplink"  />

						<domain name="uplink">
							<nat domain="downlink" icmp-ids="999"/>
						</domain>

						<domain name="downlink" interface="10.0.1.79/24">
							<dhcp-server ip_first="10.0.1.80" ip_last="10.0.1.100"/>
							<icmp dst="0.0.0.0/0" domain="uplink" />
						</domain>

					</config>

				</inline>
				<sleep milliseconds="3007"/>
				<inline>

					<config dhcp_discover_timeout_sec="1"
					        verbose="}              [router_verbose] {"
					        verbose_packet_drop="}  [router_verbose_packet_drop] {"
					        verbose_domain_state="} [router_verbose_domain_state] {"
					        verbose_packets="}      [router_verbose_packets] {">

						<policy label_prefix="ping"    domain="downlink"/>
						<policy label_prefix="nic_drv" domain="uplink"  />

						<domain name="uplink">
							<nat domain="downlink" icmp-ids="999"/>
						</domain>

						<domain name="downlink" interface="10.0.1.79/24">
							<dhcp-server ip_first="10.0.1.80" ip_last="10.0.1.100"/>
							<icmp dst="0.0.0.0/0" domain="uplink" />
						</domain>

					</config>

				</inline>
				<sleep milliseconds="3008"/>
				<inline>

					<config dhcp_discover_timeout_sec="1"
					        verbose="}              [router_verbose] {"
					        verbose_packet_drop="}  [router_verbose_packet_drop] {"
					        verbose_domain_state="} [router_verbose_domain_state] {"
					        verbose_packets="}      [router_verbose_packets] {">

						<policy label_prefix="ping" domain="downlink"/>

						<domain name="downlink" interface="10.0.1.79/24">
							<dhcp-server ip_first="10.0.1.80" ip_last="10.0.1.100"/>
						</domain>

					</config>

				</inline>
				<sleep milliseconds="600000"/>
			</rom>
		</config>
	</start>

	<start name="router" caps="200" priority="-2">
		<binary name="nic_router"/>
		<resource name="RAM" quantum="10M"/>
		<provides>
			<service name="Nic"/>
			<service name="Uplink"/>
		</provides>
		<route>
			<service name="ROM" label="config">
				<child name="dynamic_rom" label="router.config"/>
			</service>
			<any-service> <parent/> <any-child/> </any-service>
		</route>
	</start>

	<start name="ping" priority="-2">
		<resource name="RAM" quantum="8M"/>
		<config dst_ip="1.1.1.1"
		        period_sec="1"
		        count="999"/>
		<route>
			<service name="Nic"> <child name="router"/> </service>
			<any-service> <parent/> <any-child/> </any-service>
		</route>
	</start>

</config>
}

install_config $config

append boot_modules {
	iwlwifi-6000-4.ucode
	iwlwifi-6000g2a-6.ucode
	iwlwifi-6000g2b-6.ucode
	iwlwifi-7260-17.ucode
	iwlwifi-7265-17.ucode
	iwlwifi-7265D-29.ucode
	iwlwifi-8000C-36.ucode
	iwlwifi-8265-36.ucode
	regulatory.db
}

append boot_modules { report_rom }
append boot_modules { vfs_jitterentropy.lib.so }
append boot_modules { libcrypto.lib.so }
append boot_modules { libssl.lib.so }
append boot_modules { wpa_driver_nl80211.lib.so }
append boot_modules { wpa_supplicant.lib.so }
append boot_modules { wifi.lib.so }
append boot_modules { wifi_drv }
append boot_modules { core }
append boot_modules { nic_router }
append boot_modules { ld.lib.so }
append boot_modules { init }
append boot_modules { timer }
append boot_modules { ping }
append boot_modules { libc.lib.so }
append boot_modules { dynamic_rom }
append boot_modules { rtc_drv }
append boot_modules { vfs.lib.so }
append boot_modules { ipxe_nic_drv }
append_platform_drv_boot_modules

build_boot_image $boot_modules

append done_string ".*router.config: change"
append done_string ".*router.config: sleep 3001 milliseconds"
append done_string ".*64 bytes from 1.1.1.1: icmp_seq="

append done_string ".*router.config: change"
append done_string ".*router.config: sleep 3002 milliseconds"
append done_string ".*64 bytes from 1.1.1.1: icmp_seq="

append done_string ".*router.config: change"
append done_string ".*router.config: sleep 3003 milliseconds"
append done_string ".*downlink.*invalid domain.*invalid ICMP rule"

append done_string ".*router.config: change"
append done_string ".*router.config: sleep 3004 milliseconds"
append done_string ".*64 bytes from 1.1.1.1: icmp_seq="

append done_string ".*router.config: change"
append done_string ".*router.config: sleep 3005 milliseconds"
append done_string ".*64 bytes from 1.1.1.1: icmp_seq="

append done_string ".*router.config: change"
append done_string ".*router.config: sleep 3006 milliseconds"
append done_string ".*downlink.*invalid domain.*invalid ICMP rule"

append done_string ".*router.config: change"
append done_string ".*router.config: sleep 3007 milliseconds"
append done_string ".*64 bytes from 1.1.1.1: icmp_seq="

append done_string ".*router.config: change"
append done_string ".*router.config: sleep 3008 milliseconds"
append done_string ".*64 bytes from 1.1.1.1: icmp_seq="

append done_string ".*router.config: change"
append done_string ".*router.config: sleep 600000 milliseconds"
append done_string ".*From 10.0.1.79 icmp_seq=.* Destination Unreachable"

run_genode_until $done_string 70
