set use_sd_card_drv [expr [have_spec pbxa9]]
set use_ahci_drv    [expr [have_spec x86] && ![have_spec linux]]
set use_vfs_block   [have_spec linux]

if {[expr ![have_include "power_on/qemu"] && !$use_vfs_block]} {
	puts "\nPlease setup your native sd or hard drive. Remove this fail stop";
	puts "check when you have prepared your native environment.\n";
	exit 0
}


#
# Build
#

set build_components {
	core init timer
	test/libc_block
}

lappend_if $use_ahci_drv    build_components drivers/ahci
lappend_if $use_sd_card_drv build_components drivers/sd_card
lappend_if $use_vfs_block   build_components server/vfs_block
lappend_if $use_vfs_block   build_components lib/vfs/import

source ${genode_dir}/repos/base/run/platform_drv.inc
append_platform_drv_build_components

build $build_components
create_boot_directory

#
# Generate config
#

set config {
<config verbose="yes">
	<parent-provides>
		<service name="ROM"/>
		<service name="IRQ"/>
		<service name="IO_MEM"/>
		<service name="IO_PORT"/>
		<service name="PD"/>
		<service name="RM"/>
		<service name="CPU"/>
		<service name="LOG"/>
	</parent-provides>
	<default-route>
		<any-service> <parent/> <any-child/> </any-service>
	</default-route>
	<default caps="100"/>
	<start name="timer">
		<resource name="RAM" quantum="1M"/>
		<provides> <service name="Timer"/> </provides>
	</start>
	<start name="test-libc_block">
		<resource name="RAM" quantum="2M"/>
		<config>
			<libc stdout="/dev/log"/>
			<vfs>
				<dir name="dev">
					<log/>
					<block name="blkdev"/>
				</dir>
			</vfs>
		</config>
	</start>}

append_platform_drv_config

append_if $use_ahci_drv config {
	<start name="ahci_drv">
		<resource name="RAM" quantum="10M"/>
		<provides> <service name="Block"/> </provides>
		<config ata="yes">
			<policy label_prefix="test-libc_block" device="0"/>
		</config>
	</start>
}

append_if $use_sd_card_drv config {
	<start name="pbxa9_sd_card_drv">
		<resource name="RAM" quantum="1M" />
		<provides><service name="Block"/></provides>
	</start>
}

append_if $use_vfs_block config {
	<start name="vfs_block">
		<resource name="RAM" quantum="68M"/>
		<provides><service name="Block"/></provides>
		<config>
			<vfs>
				<ram/>
				<import>
					<zero name="test.hda" size="64M"/>
				</import>
			</vfs>
			<default-policy file="/test.hda" block_size="512"
			                writeable="yes"/>
		</config>
	</start>}

append config {
</config>
}

install_config $config

#
# Boot modules
#

# generic modules
set boot_modules {
	core init timer
	ld.lib.so libc.lib.so vfs.lib.so libm.lib.so posix.lib.so
	test-libc_block
}

lappend_if $use_ahci_drv     boot_modules ahci_drv
lappend_if $use_sd_card_drv  boot_modules pbxa9_sd_card_drv
lappend_if $use_vfs_block    boot_modules vfs_block
lappend_if $use_vfs_block    boot_modules vfs_import.lib.so

append_platform_drv_boot_modules

build_boot_image $boot_modules

#
# Execute test case
#

set disk_image "bin/test.hda"
set cmd "dd if=/dev/zero of=$disk_image bs=1024 count=65536"
puts "creating disk image: $cmd"
catch { exec sh -c $cmd }

#
# Qemu
#
append qemu_args "  -nographic "
append_if $use_ahci_drv    qemu_args " -drive id=disk,file=$disk_image,format=raw,if=none -device ahci,id=ahci -device ide-drive,drive=disk,bus=ahci.0 -boot d"
append_if $use_sd_card_drv qemu_args " -drive file=$disk_image,format=raw,if=sd,cache=writeback "

run_genode_until {.*child "test-libc_block" exited with exit value 0.*} 60

exec rm -f $disk_image

puts "\nTest succeeded\n"

# vi: set ft=tcl :
