#
# \brief  Test for using the lwIP TCP/IP stack
# \author Norman Feske
# \date   2011-05-22
#
# This test case executes a small HTTP server on Genode running on qemu. When
# the HTTP server is up, a HTTP request to the server is performed using
# 'lynx'. The response is validated against a known pattern.
#
# The test uses qemu's "-netdev user" option, redirecting Genode's port 80 to the
# host's port 5555. Consequently, it cannot be executed on non-qemu test
# environments (i.e., the test won't work with the Linux version of Genode).
#
# Please make sure to include a nic driver in your build configuration. E.g.,
# on the x86 platform, you may enable the 'dde_ipxe' repository.
#

#
# TODO: Add support for Linux via user-level networking (using the
#       tun/tap proxy driver at os/src/drivers/nic/linux)
#

if {[expr [have_spec linux]] ||
    [expr [have_spec imx53] && [have_spec trustzone]] ||
    [have_spec rpi3] ||
    [expr [have_spec riscv]]} {
	puts "\n Run script is not supported on this platform. \n"; exit 0 }

set lynx [installed_command lynx]

create_boot_directory

import_from_depot [depot_user]/src/[base_src] \
                  [depot_user]/pkg/[drivers_nic_pkg] \
                  [depot_user]/src/init \
                  [depot_user]/src/libc \
                  [depot_user]/src/vfs_lwip \
                  [depot_user]/src/vfs

install_config {
<config verbose="yes" prio_levels="2">
	<parent-provides>
		<service name="ROM"/>
		<service name="IRQ"/>
		<service name="IO_MEM"/>
		<service name="IO_PORT"/>
		<service name="PD"/>
		<service name="RM"/>
		<service name="CPU"/>
		<service name="LOG"/>
	</parent-provides>
	<default-route>
		<any-service> <parent/> <any-child/> </any-service>
	</default-route>
	<default caps="100"/>

	<start name="timer">
		<resource name="RAM" quantum="1M"/>
		<provides> <service name="Timer"/> </provides>
	</start>

	<start name="drivers" caps="1000" managing_system="yes" priority="-1">
		<resource name="RAM" quantum="32M"/>
		<binary name="init"/>
		<route>
			<service name="ROM" label="config"> <parent label="drivers.config"/> </service>
			<service name="Timer"> <child name="timer"/> </service>
			<any-service> <parent/> </any-service>
		</route>
		<provides> <service name="Nic"/> </provides>
	</start>

	<start name="test-lwip_httpsrv" caps="120" priority="-1">
		<resource name="RAM" quantum="4M"/>
		<config>
			<vfs>
				<dir name="dev">    <log/>             </dir>
				<dir name="socket"> <lwip dhcp="yes"/> </dir>
			</vfs>
			<libc stdout="/dev/log" stderr="/dev/log" socket="/socket"/>
		</config>
	</start>
</config>
}

build { test/lwip/http_srv }

build_boot_image { test-lwip_httpsrv }

#
# Qemu config
#
append qemu_args "  -nographic "
append_qemu_nic_args "hostfwd=tcp::5555-:80"

run_genode_until {.*Start the server loop.*\n} 30

if {[have_include "power_on/qemu"]} {
	set uri "http://localhost:5555/"
} else {
	set match_string "lwIP Nic interface up address=.* netmask.*\n"
	regexp $match_string $output ip_addr
	regexp {[0-9]+\.[0-9]+\.[0-9]+\.[0-9]+} $ip_addr ip_addr 

	set uri "http://$ip_addr:80/"
}

puts "http server is up, try to query website $uri"

set website [exec $lynx -dump $uri]

puts "response:\n$website"

if {![regexp {Welcome to our lwIP HTTP server!} $website dummy]} {
	puts stderr "Query returned unexpected website"
	exit 2;
}

# vi: set ft=tcl :
