#
# Build components
#

proc test_timeout { } {
	if {[have_spec foc] && [have_spec x86_64] && [have_include power_on/qemu]} {
		return 150
	} else {
		return 60
	}
}

proc enable_test_1 { } { return 1 }
proc enable_test_2 { } { return 1 }
proc enable_test_3 { } { return 1 }
proc enable_test_4 { } { return 1 }
proc enable_test_5 { } { return 1 }
proc enable_test_6 { } { return 1 }
proc enable_test_7 { } { return 1 }

source ${genode_dir}/repos/libports/run/nic_router.inc

lappend targets server/report_rom

build $targets

create_boot_directory


#
# Test 1 utilities
#

proc test_1_config { } {
	if {[enable_test_1]} { return "
		[client_config t1_d1_c1_udp udp 10.0.98.55 10.0.98.33 255.255.255.0 nic_router 1337 10.0.98.33]
		[client_config t1_d2_c1_udp udp 10.0.99.56 10.0.99.33 255.255.255.0 nic_router  999 10.0.99.55]
		[server_config t1_d2_s1_udp udp 10.0.99.55 10.0.99.33 255.255.255.0 nic_router  999 ]" }
}

proc test_1_router_config { } {
	if {[enable_test_1]} { return {
		<policy label_prefix="t1_d1" domain="t1_d1" />
		<policy label_prefix="t1_d2" domain="t1_d2" />

		<domain name="t1_d1" interface="10.0.98.33/24">
			<udp-forward port="1337" domain="t1_d2" to="10.0.99.55" to_port="999" />
		</domain>

		<domain name="t1_d2" interface="10.0.99.33/24" />} }
}

proc test_1_router_uplink_config { } { }


#
# Test 2 utilities
#

proc test_2_config { } {
	if {[enable_test_2]} { return "
		[client_config t2_d0_c1_udp udp 10.0.2.212  10.0.2.1    255.255.255.0 nic_bridge 1 10.0.2.55]
		[server_config t2_d1_s1_udp udp 18.17.16.15 18.17.16.14 255.255.0.0   nic_router 1 ]" }
}

proc test_2_router_config { } {
	if {[enable_test_2]} { return {
		<policy label_prefix="t2_d1" domain="t2_d1" />
		<domain name="t2_d1" interface="18.17.16.14/24" />} }
}

proc test_2_router_uplink_config { } {
	if {[enable_test_2]} { return {
		<udp-forward port="1" domain="t2_d1" to="18.17.16.15" />} }
}


#
# Test 3 utilities
#

proc test_3_config { } {
	if {[enable_test_3]} { return "
		[client_config t3_d1_c1_udp udp 217.13.192.2 217.13.192.1 255.255.192.0 nic_router 65535 10.0.2.213]
		[server_config t3_d0_s1_udp udp 10.0.2.213   10.0.2.55    255.255.255.0 nic_bridge 65535 ]" }
}

proc test_3_router_config { } {
	if {[enable_test_3]} { return {
		<policy label_prefix="t3_d1" domain="t3_d1" />

		<domain name="t3_d1" interface="217.13.192.1/24">
			<ip dst="10.0.2.0/24" domain="uplink" />
		</domain>} }
}

proc test_3_router_uplink_config { } {
	if {[enable_test_3]} { return {
		<ip dst="217.13.192.0/24" domain="t3_d1" />} }
}


#
# Test 4 utilities
#

proc test_4_config { } {
	if {[enable_test_4]} { return "
		[client_config t4_d0_c1_tcp http 10.0.2.201   10.0.2.1    255.255.255.0 nic_bridge 80   10.0.2.55]
		[server_config t4_d1_s1_tcp http 192.168.1.18 192.168.1.1 255.255.255.0 nic_router 2048 ]" }
}

proc test_4_router_config { } {
	if {[enable_test_4]} { return {
		<policy label_prefix="t4_d1" domain="t4_d1" />
		<domain name="t4_d1" interface="192.168.1.1/24" />} }
}

proc test_4_router_uplink_config { } {
	if {[enable_test_4]} { return {
		<tcp-forward port="80" domain="t4_d1" to="192.168.1.18" to_port="2048" />} }
}

#
# Test 5 utilities
#

proc test_5_config { } {
	if {[enable_test_5]} { return "
		[client_config t5_d0_c1_tcp http 10.0.2.202   10.0.2.1    255.255.255.0 nic_bridge 8080 10.0.2.55]
		[server_config t5_d1_s1_tcp http 192.168.2.72 192.168.2.1 255.255.255.0 nic_router 8080 ]" }
}

proc test_5_router_config { } {
	if {[enable_test_5]} { return {
		<policy label_prefix="t5_d1" domain="t5_d1" />
		<domain name="t5_d1" interface="192.168.2.1/24" />} }
}

proc test_5_router_uplink_config { } {
	if {[enable_test_5]} { return {
		<tcp-forward port="8080" domain="t5_d1" to="192.168.2.72" />} }
}


#
# Test 6 utilities
#

proc test_6_config { } {
	if {[enable_test_6]} { return "
		[client_config t6_d1_c1_tcp http 100.200.0.128 100.200.0.1 255.255.0.0   nic_router 2345 10.0.2.203]
		[server_config t6_d0_s1_tcp http 10.0.2.203    10.0.2.1    255.255.255.0 nic_bridge 2345 ]" }
}

proc test_6_router_config { } {
	if {[enable_test_6]} { return {
		<policy label_prefix="t6_d1" domain="t6_d1" />

		<domain name="t6_d1" interface="100.200.0.1/24">
			<tcp dst="10.0.0.0/16">
				<permit port="2345" domain="uplink" />
			</tcp>
		</domain>} }
}

proc test_6_router_uplink_config { } {
	if {[enable_test_6]} { return {
		<nat domain="t6_d1" tcp-ports="6" />} }
}


#
# Test 7 utilities
#

proc test_7_config { } {
	if {[enable_test_7]} {

		append config "
			[client_config t7_d1_c1_tcp http dhcp       dhcp     dhcp          t7_d1_nic_router 2345 10.0.2.204]
			[client_config t7_d1_c2_tcp http dhcp       dhcp     dhcp          nic_router       3456 10.0.2.240]
			[client_config t7_d1_c3_tcp http dhcp       dhcp     dhcp          nic_router       3456 10.0.2.240]
			[server_config t7_d2_s1_tcp http 10.0.2.204 10.0.2.1 255.255.255.0 nic_router       2345 ]
			[server_config t7_d2_s2_tcp http 10.0.2.240 10.0.2.1 255.255.255.0 nic_router       3456 ]"

		append config {
			<start name="t7_d1_nic_router" caps="200" priority="-1">
				<binary name="nic_router"/>
				<resource name="RAM" quantum="10M"/>
				<provides><service name="Nic"/></provides>
				<config>

					<policy label_prefix="t7_d1" domain="downlink" />
					<uplink                      domain="uplink"   />

					<domain name="uplink">
						<nat domain="downlink" tcp-ports="6" />
					</domain>

					<domain name="downlink" interface="100.2.3.1/24">
						<dhcp-server ip_first="100.2.3.2"
						             ip_last="100.2.3.10"
						             dns_server_from="uplink"/>

						<tcp dst="10.0.0.0/16">
							<permit port="2345" domain="uplink" />
						</tcp>
					</domain>

				</config>
				<route>
					<service name="Nic"> <child name="nic_router"/> </service>
					<service name="Report"> <child name="report_rom"/> </service>
					<any-service> <parent/> <any-child/> </any-service>
				</route>
			</start>}

		return $config
	}
}

proc test_7_router_config { } {
	if {[enable_test_7]} { return {
		<policy label_prefix="t7_d1" domain="t7_d1" />
		<policy label_prefix="t7_d2" domain="t7_d2" />

		<domain name="t7_d1" interface="100.200.0.1/24">
			<dhcp-server ip_first="100.200.0.32"
			             ip_last="100.200.0.64"
			             ip_lease_time_sec="3600"
			             dns_server="8.8.8.8"/>

			<tcp dst="10.0.0.0/16">
				<permit port="2345" domain="t7_d2" />
				<permit port="3456" domain="t7_d2" />
			</tcp>
		</domain>

		<domain name="t7_d2" interface="10.0.2.1/24">
			<nat domain="t7_d1" tcp-ports="18" />
		</domain>} }
}

proc test_7_router_uplink_config { } { }


#
# Init config
#

append config {
<config prio_levels="2">
	<parent-provides>
		<service name="ROM"/>
		<service name="IRQ"/>
		<service name="IO_MEM"/>
		<service name="IO_PORT"/>
		<service name="PD"/>
		<service name="RM"/>
		<service name="CPU"/>
		<service name="LOG"/>
	</parent-provides>

	<default-route>
		<any-service> <parent/> <any-child/> </any-service>
	</default-route>

	<default caps="200"/>

	} [platform_drv_config] {

	<start name="timer" priority="0">
		<resource name="RAM" quantum="1M"/>
		<resource name="CPU" quantum="5"/>
		<provides><service name="Timer"/></provides>
	</start>

	<start name="nic_loopback" priority="-1">
		<resource name="RAM" quantum="1M"/>
		<provides> <service name="Nic"/> </provides>
	</start>

	<start name="nic_router" caps="400" priority="-1">
		<resource name="RAM" quantum="10M"/>
		<provides><service name="Nic"/></provides>
		<config verbose="no"
		        verbose_packets="no"
		        verbose_domain_state="yes"
		        dhcp_discover_timeout_sec="3"
		        dhcp_request_timeout_sec="3"
		        dhcp_offer_timeout_sec="3"
		        udp_idle_timeout_sec="30"
		        tcp_idle_timeout_sec="30"
		        tcp_max_segm_lifetime_sec="15">

			<report bytes="yes"
			        config="yes"
			        quota="no"
			        stats="no"
			        link_state="yes"
			        link_state_triggers="yes"
			        interval_sec="60" />

			<uplink domain="uplink"/>

			<domain name="uplink"
			        interface="10.0.2.55/24"
			        gateway="10.0.2.1"
			        verbose_packets="no">

				} [test_1_router_uplink_config] {
				} [test_2_router_uplink_config] {
				} [test_3_router_uplink_config] {
				} [test_4_router_uplink_config] {
				} [test_5_router_uplink_config] {
				} [test_6_router_uplink_config] {
				} [test_7_router_uplink_config] {

			</domain>

			} [test_1_router_config] {
			} [test_2_router_config] {
			} [test_3_router_config] {
			} [test_4_router_config] {
			} [test_5_router_config] {
			} [test_6_router_config] {
			} [test_7_router_config] {

		</config>
		<route>
			<service name="Nic"> <child name="nic_bridge"/> </service>
			<service name="Report"> <child name="report_rom"/> </service>
			<any-service> <parent/> <any-child/> </any-service>
		</route>
	</start>

	<start name="nic_bridge" caps="200" priority="-1">
		<resource name="RAM" quantum="10M"/>
		<provides><service name="Nic"/></provides>
		<config>
			<policy label_prefix="nic_router"   ip_addr="10.0.2.55"  />
			<policy label_prefix="t2_d0_c1_udp" ip_addr="10.0.2.212" />
			<policy label_prefix="t3_d0_s1_udp" ip_addr="10.0.2.213" />
			<policy label_prefix="t4_d0_c1_tcp" ip_addr="10.0.2.201" />
			<policy label_prefix="t5_d0_c1_tcp" ip_addr="10.0.2.202" />
			<policy label_prefix="t6_d0_s1_tcp" ip_addr="10.0.2.203" />
		</config>
		<route>
			<service name="Nic"> <child name="nic_loopback"/> </service>
			<any-service> <parent/> <any-child/> </any-service>
		</route>
	</start>

	<start name="report_rom">
		<resource name="RAM" quantum="1M"/>
		<provides> <service name="Report"/> <service name="ROM"/> </provides>
		<config verbose="yes"/>
	</start>

	} [test_1_config] {
	} [test_2_config] {
	} [test_3_config] {
	} [test_4_config] {
	} [test_5_config] {
	} [test_6_config] {
	} [test_7_config] {

</config> }

install_config $config

lappend boot_modules report_rom

build_boot_image $boot_modules

for {set i 0} {$i < $nr_of_clients} {incr i 1} {
	append done_string {.*Test done.*\n}
}

run_genode_until $done_string [test_timeout]
